Home Maintenance Calendar
A little regular maintenance prevents most expensive repairs. Tick each job off as you go.
Spring
	☐
	Look over the roof from the ground for slipped or missing tiles after the winter.

	☐
	Check gutters and downpipes are clear and not leaking at the joints.

	☐
	Check fences, gates and garden walls after the winter winds.

	☐
	Look for damp patches inside, especially below windows and on chimney breasts.

	☐
	Make sure air bricks are clear of soil, plants and rubbish.


Summer
	☐
	Repaint or treat outside woodwork and metalwork while the weather is dry.

	☐
	Check pointing and render for cracks or loose areas.

	☐
	Cut back plants and ivy growing on walls, and keep trees near the house in check.

	☐
	Check drains and gullies are clear and flowing freely.

	☐
	Have chimneys swept before the heating season if you use an open fire or wood burner.


Autumn
	☐
	Clear the gutters once the leaves have fallen.

	☐
	Have the boiler serviced by a Gas Safe registered engineer.

	☐
	Bleed the radiators and check the heating works before the cold weather.

	☐
	Check pipes and tanks in the loft are lagged, and the loft insulation is in place.

	☐
	Turn off and drain outside taps, or fit covers.


Winter
	☐
	Know where your stopcock is, and check it turns.

	☐
	Keep the heating on low if you're away, to stop pipes freezing.

	☐
	Check the loft after storms for leaks or daylight through the roof.

	☐
	Open windows or use extractor fans to keep condensation down.


All year round
	☐
	Test smoke and carbon monoxide alarms every month.

	☐
	Look out for new or widening cracks in walls. If you find one, have it checked.

	☐
	Deal with small leaks and blocked gutters straight away, before they cause bigger damage.


Stay safe: don't work on roofs or gutters, or from a ladder at height, yourself. Look from the ground, and use a contractor with proper access equipment for anything above.
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